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ATF SPECIAL
ATF SPECIAL is formulated with synthetic base oil and advanced additive technology to meet the challenging demands of an automatic transmission environment. 

ATF SPECIAL is a high quality friction modified lubricant qualified by both General Motors and Ford. Its responsive low temperature fluidity is beneficial in both electronic and hydraulic controlled transmissions and transaxles. It may be used for service fill where Mercon, Dexron, Dexron II or Dexron IIE is recommended. ATF SPECIAL meets the latest “H” version of the licensing. 
ATF SPECIAL is recommended for lock-up clutch vehicles. 
Benefits of ATF SPECIAL include :

• Contains extreme pressure performance ensuring excellent protection gears from wearing and longer gear life.
• Excellent thermal and oxidation stability for long and consistent transmission performance.
• Effective foam control properties provide consistent shifting performance.

	Performance Level

	Dexron III(H)
Ford Mercon
Hyundai/ KIA SP-Ⅱ, Hyundai/ KIA SP-Ⅲ


	Typical Properties
	
	

	Specific Gravity (15/4℃)
	
	0.8572

	Kinematic Viscosity (100℃, cSt)
	
	6.514

	Kinematic Viscosity (40℃, cSt)
	
	31.48

	Viscosity Index 
	
	167

	Flash Point (℃)
	
	210

	Pour Point (℃)
	
	-45.0


· Values shown are typical and may vary

